Check flag = 1

Led On

Yes

Send data to the second micro

Send to the first micro

Read the Bluetooth terminal Data

Initialize Bluetooth

Start